[bookmark: et]Basic Status
[bookmark: t_devinfo]Device Information
[bookmark: t_swver][bookmark: sver]Firmware Version:0.6.0 0.4 v0005.0 Build 130217 Rel.62075n
[bookmark: t_hwver][bookmark: hver]Hardware Version:TD-W8968 v1 00000000
[bookmark: t_uptime][bookmark: UpTime]System up time:27 day(s) 05:06:29

DSL
[bookmark: t_link][bookmark: dslstatus]Line Status:Connected
[bookmark: t_dslmode][bookmark: modulationType]DSL Modulation Type:ADSL_2plus
[bookmark: t_annex][bookmark: annexMode]Annex Type:Annex A/I/J/L/M
[bookmark: dslTbl][bookmark: dslTbl]
	[bookmark: t_up] 
	[bookmark: t_down]Upstream
	Downstream

	[bookmark: t_currate]Current Rate (Kbps)
	[bookmark: upstreamCurrRate]1020
	[bookmark: downstreamCurrRate]8192

	[bookmark: t_maxrate]Max Rate (Kbps)
	[bookmark: upstreamMaxRate]1076
	[bookmark: downstreamMaxRate]14608

	[bookmark: t_snr]SNR Margin (dB)
	[bookmark: upstreamNoiseMargin]7.4
	[bookmark: downstreamNoiseMargin]11

	[bookmark: t_att]Line Attenuation (dB)
	[bookmark: upstreamAttenuation]13.9
	[bookmark: downstreamAttenuation]29

	[bookmark: t_errs]Errors (Pkts)
	[bookmark: UCRC]0
	[bookmark: DCRC]0



WAN
[bookmark: wan_table][bookmark: wan_table]
	[bookmark: t_title]Name
	Connection Type
	VPI/VCI
	IP/Mask
	Gateway
	DNS
	Status

	pppoa_0_38_0_d
	PPPoA
	0/38
	92.18.44.9 /32
	92.18.32.1
	62.24.134.5 78.151.235.4
	Connected



IPv6 WAN
[bookmark: wan6_table][bookmark: wan6_table]
	[bookmark: t_ip6title]Name
	Connection Type
	[bookmark: t_ip6addrplen]VPI/VCI
	IPv6 Address/Prefix Length
	Gateway
	DNSv6
	Status



LAN

[bookmark: lanmac]MAC Address:A0:F3:C1:4F:D8:AC
[bookmark: lanip]IP Address:192.168.1.1
[bookmark: lanmask]Subnet Mask:255.255.255.0
[bookmark: dhcpen]DHCP:Enabled

IPv6 LAN

[bookmark: lan6addr]IPv6 Address:N/A
[bookmark: lan6prelen]Prefix Length:64
[bookmark: t_lan6cfgtype][bookmark: cfgtype]Autoconfiguration Type:RADVD

Wireless

[bookmark: wlstat]Status:Enabled
[bookmark: wlssid]SSID:Shapwick2
[bookmark: wlchl]Channel:Auto(Channel 1)
[bookmark: wlbw]Channel Width:Auto
[bookmark: wlmod]Mode:11bgn mixed
[bookmark: wlenc]Encryption:WPA-PSK/WPA2-PSK
[bookmark: wlmac]MAC Address:A0:F3:C1:4F:D8:AC
[bookmark: t_tx1][bookmark: wlrate]Max Tx Rate:300Mbps
[bookmark: t_wlwds][bookmark: wlwds]WDS Status:Disabled




[bookmark: title_sysMode][bookmark: et1]Operation Mode[image: ]
[bookmark: t_mode]Choose Operation Mode:
[bookmark: sysmod1]ADSL Modem Router Mode  --this one
[bookmark: sysmod4]3G Router Mode 
[bookmark: sysmod2]Wireless Router Mode
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DSL Modulation Type:
Annex Type:

Auto Sync-up

Annex A//J/LM

© Enable Bit Swap
(& Enable SRA
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DHCP Settings

This page allows you to set DHCP server which provides TCP/IP configuration for all the PCs connected to the Modem Router in the LAN.

Group: Default
IP Address: 192.168.1.1
Subnet Mask: 255.255.255.0
DHCP Server: O Disable ® Enable O DHCP Relay

Start IP Address: [152-168-1.100
End IP Address: [192.162.1.199
Lease Time: [1:20 minutes (1~2880 minutes, the default value is 1440)
Default Gateway: [1s2.162.1.1  (optional)
Default Domain: [ (optional)
DNS Server: [e2.2:.132.1  (optional)
Secondary DNS Server: [0.c.0.0  (optional)
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DHCP Clients List

This page displays the information of DHCP clients.

D Client Name MAC Address IP Address Valid Time
1 a"d""d':?gudfs“s 84:38:38:F7:8C:TF 192.168.1.105 17:16:52
2 Unknown B4:07:F9:E3:1D:7E 192.168.1.100 23:57:22
3 ColinM-PC D0:27:88:A9:F7:A1 192.168.1.107 16:06:03
4 NPI465423 F4:CE:46:46:54:23 192.168.1.108 15:58:08
5 DESKTOP-SIALK5T 98:5F:D3:3C:C7:D5 192.168.1.103 20:23:00
6 Unknown ©C:2D:8C:36:30:FD 192.168.1.104 05:38:36
7 TL-WAB0IND F4:F2:6D:59:C8:A6 192.168.1.113 04:09:35
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DHCP Address Reservation

This page displays the static IP assigned by DHCP Server and allows you to configure it by clicking corresponding buttons.

a MAC Address IP Address Group Status Edit

Add New Enable Selected Disable Selected Delete Selected
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DHCP C nal Pool

This page displays vendor class settings and allows you to set parameters for vendor class by clicking corresponding buttons.

Start IP Address/ End IP - "
a Vendor ID Address Facility Group Status Edit
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reless Basic Settings

Wireless: @ Enable O Disable
SSID:  [shapviciz

Region: [UntedKngdom v

Warning:  Ensure you select a correct country to conform local law.
Incorrect settings may cause interference.
Mode: [ 11bon mied <
Channel: | Auto 4
Channel Width: | Auto &

M Enable SSID Broadcast
O Enable WDS
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WPS Settings

WPS:  Disabled
Curent N 75124878 [ s | [ i
Add a new device: | i |




image16.png
eless Security Settings

For network security, it is strongly recommended to enable wireless security and use WPA2-PSK AES encryption.

O Disable Wireless Security

@® WPA/WPA2 - Personnal (Recommended)

Authentication Type:
Encryption:
Wireless Password:

Group Key Update Period:

O WPA/WPA2 - Enterprise

Authentication Type:
Encryption:

RADIUS Server IP:
RADIUS Server Port:
RADIUS Server Password:

Group Key Update Period:

O WEP

Authentication Type:
WEP Key Format:
Selected Key:

Key 1:
Key 2:
Key 3:
Key 4:

WPAZPSK

AES

[shapwicksosozer
(Enter ASCII characters between 8 and 63 or Hexadecimal characters between 8 and 64.)

0 (seconds, minimum is 30, 0 means no update)

(Enter ASCII characters between 8 and 63 or Hexadecimal characters between 8 and 64.)

0 (in second, minimum is 30, 0 means no update)

Open System

Hexadecmal

WEP Key

Disabled

Disabled

Disabled

Disabled

Key Type
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Wireless MAC Filteri

g settings

‘You can configure the Wireless MAC Filtering to control the wireless access on this page.

Wireless MAC Filtering: Disabled

Filtering Rules

@ Deny the stations specified by any enabled entries in the list to access.
OAllow the stations specified by any enabled entries in the list to access.

Enable

o

MAC Address

Status

Edit

Enable Selected
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Wirelsss Lan Advanced Settings

Transmit Power: [ 100% [
Beacon Interval: [100  (25-1000)
RTS Threshold: [z (1-2346)
Fragmentation Threshold: [23:c  (256-2346)
DTIMInterval: [t (1-255)
& Enable Short GI
O Enable Client isolation
' Enable WMM
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Operation Mode

Choose Operation Mode:

@ ADSL Modem Router Mode
O 3G Router Mode
O Wireless Router Mode
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Wireless Stations Stat

This page displays the basic information of all stations in this wireless network.

Current Connected Wireless Stations numbers: 2 Refresh

=} MAC Address Current Status Received Packets Sent Packets
1 84:38:38:F7:8C:7F Associated 1883 2087
2 98:5F:D3:3C:C7:D5 Associated 4049 1268





image2.png
SL WAN Interface

This page shows the information of the entire ADSL WAN interface.

Name Type VPIVCI| IPv4 1Pv6 IP/Mask Gateway DNS Status Connect Action
pppoa_0_38_0_d | PPPoA | 0/38 | Enable | Disable | 92.18.44.9/32 | 92.18.32.1 768212;1::554 Connected Disconnect Edit Delete
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3G settings is unavailable because the operation mode is not 3G Router Mode and the backup is not enabled. Please Enable 3G backup or
change settings on Operation Mode if you want to use 3G.

[ Enable 3G as a backup solution for Internet access
USB 3G modem: Unplugged
PIN status: Unknown

Location: | usa 2
Mobile ISP: | AT&T

Connection Mode: Always on
Connect on demand
Connect manually
Max Idle Time:[i5~ minutes (0 means remain active at all times)

Authentication Type: [suroaum

Connect | Disconnect Disconnected





image4.png
Interface Grouping

This page displays all the current groups.
Note: It is not allowed to disable the VLAN with Ethernet WAN Connection enabled.

VLAN: O Enable ® Disable Save

Group Delete WAN Interface LAN Interface
LAN
Default
ra0
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LAN Settings

Note: If the LAN IP address or subnet mask is changed, please make sure the DHCP Address Pool and the static IP assigned by DHCP Server are
in the same subnet with the new LAN IP.

Group:  Default
IP Address: [TZ-168.11
Subnet Mask: [255-255.255.0

Enable IGMP Snooping: O
Enable Second IP: O

DHCP Server: O Disable ® Enable O DHCP Relay
Start IP Address:  |192-168.1.100
End IP Address: [192.162.1.15%

Leased Time: [1:20 minutes (1~2880 minutes, the default value is 1440)
Gateway: [1s2.162.1.1  (optional)
Default Domain: [ (optional)
DNS Server: [s2.2:6.135.1  (optional)
Secondary DNS Server: [0.0.0.0  (optional)
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IPv6 LAN Settings

The parameters of IPv6 LAN can be configured on this page.
Note: Only default group supports IPv6 now.

Group: Default
Address Autoconfiguration Type: ® RADVD O DHCPV6 Server

Site Prefix Configuration Type: @ Delegated O Static
Prefix Delegated WAN Connection: [[ho avatable interface. [+
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MAC Clone

WAN Connection MAC Address Operation
Current PC's MAC Clone MACTo | | -

Note:
1. MAC clone may cause reconnection.
2. After MAC Clone, the bridge connections sharing the same VPI/VCI with other connections may not work.
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LG Settings

Virtual Private Network(VPN):
PPTP Pass-through: @ Enable O Disable
L2TP Pass-through: @ Enable O Disable
IPSec Pass-through: @ Enable O Disable

Application Layer Gateway(ALG):
FTP ALG: @ Enable O Disable

TFTP ALG: @ Enable O Disable




